(*
  DUT: struct_room_outs
  Room light outputs (and status to Node-RED). With Option C, one set is enough:
  we send this to the relay and to Node-RED as "light status".
*)
TYPE struct_room_outs :
STRUCT
    l_1: BOOL;
    l_2: BOOL;
    l_3: BOOL;
    l_4: BOOL;
    l_5: BOOL;
    l_6: BOOL;
END_STRUCT
END_TYPE
