# LXC config (network boot: eth1 = LAN, eth0 = WAN)

Config files for the **provisioning LXC** when using **eth1** as a provisioning LAN (DHCP + TFTP for network boot, NAT for internet).

| File | Purpose |
|------|--------|
| **dnsmasq-network-boot.conf** | dnsmasq: DHCP + TFTP on eth1 only. Copied to `/etc/dnsmasq.d/` by `scripts/setup-network-boot-on-lxc.sh`. |
| **nft-nat-lan.conf** | nftables NAT so 10.20.50.0/24 uses eth0 for internet. Applied by the setup script to `/etc/nftables.d/nat-lan.conf`. |

Setup is done by running (from your machine):

```bash
./emmc-provisioning/scripts/setup-network-boot-on-lxc.sh root@<LXC-IP>
```

See [../docs/NETWORK-BOOT-LXC.md](../docs/NETWORK-BOOT-LXC.md) for full documentation.
