# Ensure CM4 boot-mode USB device is accessible to rpiboot (libusb).
# Load before 90-cm4-boot-mode.rules so permissions are set before the trigger runs.
SUBSYSTEM=="usb", ATTR{idVendor}=="2b8e", MODE="0666"
SUBSYSTEM=="usb", ATTR{idVendor}=="0a5c", ATTR{idProduct}=="2711", MODE="0666"
